{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["Sheet1","Sheet2","Sheet3","Sheet1 (2)","Sheet1 (3)"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":18,"rows_kept":16,"merged":[[0,0,0,17],[1,0,1,17]],"flags":["formulas_cached_only"]}
["建筑工程量计算程序统筹表"]
[]
[{"$nulls":6},11,"余土外运(m3)\n1-10-51-50*系数",24,"间壁墙(m2)\n间壁长*高-洞口",36,"余土外运(m3)\n31-35-51",{"$nulls":4},63,"带女儿墙屋面防水层(m2)\n61+(L中-女儿墙厚*4)*0.25"]
[{"$nulls":6},10,"地槽回填土(m3)\n1-∑基础体积及垫层(室外地坪\n以下部分)",23,"内墙勾缝(m2)\n同29",35,"地槽回填土(m3)\n31-基础体积及垫层(室外地坪下部分)",42,"外墙勾缝(m2)\nL外*勾缝高-Ⅰ-其他抹灰面",51,"地面填土(m3)\n47*填土厚",62,"带女儿墙屋顶保温层(m3)\n61*保温均厚"]
[{"$nulls":6},9,"女儿墙体积(m3)\nL中*墙高*墙厚-Ⅱ ",22,"内墙脚手架(m2)\nL内*墙高*Z",null,null,41,"外墙脚手架(m2)\nL外*砌筑高",50,"地面灰土(m3)\n47*灰土厚",61,"带女儿墙屋顶保温层上找平(m2)\nF楼-L中*女儿墙厚)"]
[{"$nulls":4},4,"基础体积(m3)\nL中*断面面积",8,"外墙体积(m3)\n(L中*层高*Z-Ⅰ)*墙厚-Ⅱ+山尖 ",21,"内墙体积(m3)\n(L内*墙高*Z-Ⅰ)*墙厚-Ⅱ+山尖",34,"基础体积(m3)\n(L内轴-两侧基础宽/2)*基础断面积",40,"圈梁露面面层(m2)\nL外*露面高*道",49,"地面垫层(m3)   地面隔热层(m3)\n47*层厚            47*层厚",60,"平屋面找平层(m2)\nF楼+41"]
[{"$nulls":4},3,"基础垫层(m3)\nL中*断面面积 ",7,"捣制砼圈梁(m3)        模板(m2)\nL中*断面面积            L中*高*2   ",20,"捣制砼圈梁(m3)      模板(m2)\nL内*断面面积          L内*高*2   ",33,"基础垫层(m3)\n(L内轴-两侧垫层宽/2)*垫层断面积",39,"腰线面层(m2)\n(L外-洞口)*展宽*道",48,"地面防潮层\n同47",59,"瓦屋面(m2)\n(F楼+外挑)*系数"]
[{"$nulls":4},2,"槽底夯实(m2)\nL中*槽底宽",6,"捣制砼地梁(m3)        模板(m2)\nL中*断面面积            L中*高*2   ",19,"捣制砼地梁(m3)      模板(m2)\nL内*断面面积          L内*高*2   ",32,"槽底夯实(m2)\n(L内轴-两侧基底宽/2)*基底宽",38,"散水(m2)\n(L外+坡宽*4-台阶)*坡宽",47,"地面面层(m2)  地面找平层(m2)\nF净                    F净",58,"龙骨吊顶(m2)\n47+52"]
[null,null,"Ⅱ","墙体内埋件\n表图示量",1,"地槽挖土(m3)\nL中*地槽断面",5,"基础防潮层(m2)\nL中*潮宽",18,"基础防潮层(m2)\nL内*潮宽",31,"地槽挖土(m3)\n(L内轴-两侧基底宽/2)*地槽断面积",37,"砼天沟挑檐面层(m2)\n(L外+檐宽*4)*檐宽","Ⅸ","F净:底层净面积(m2)\n(L中*墙厚-L内*墙厚",57,"满堂脚手架(m2)\n47+52"]
["Y","设计资料\n熟悉图纸","Ⅰ","门窗表\n图示量","Ⅲ","L中:外墙中心线(m)\n图示尺寸","Ⅳ","L外内:外墙内净长线(m)\nL中-外墙厚*4-墙厚*道","Ⅴ","L内:内墙净长线(m)\n(图示尺寸)","Ⅵ","L内轴:内墙轴线长(m)(图示尺寸)\nL内+两端1/2墙厚","Ⅶ","L外:外墙外边线(m) \n图示尺寸或L中+墙厚*4","Ⅷ","F:底层建筑面积(m2)\n图示尺寸","Ⅹ","F楼:底层建筑面积(m2)\n图示尺寸"]
[{"$nulls":6},12,"墙身防潮层(m2)\nL外内*潮高",25,"墙身防潮层(m2)\nL内*潮高*2",{"$nulls":4},46,"场地平整(m2)\nF+2*L外+16","Ⅺ","F楼净:底层净面积(m2)\n(L中*墙厚-L内*墙厚"]
[null,null,"Ⅻ","面、线外项目按图计",null,null,13,"顶棚装饰线(m) \nL外内",26,"顶棚装饰线(m)\n(L内+梁长)*2",{"$nulls":6},52,"楼面面层(m2)\nFn楼净"]
[null,null,"ⅫⅠ","其他项目按图或有关资料计算",null,null,14,"踢脚线(m) \n同13",27,"踢脚线(m)\nL内*2",null,null,43,"勒脚(m2)\n(L外-洞口)*勒脚高",null,null,53,"楼地面找平层、防潮层(m2)\n同52"]
[null,null,"ⅫⅡ","完成计算",null,null,15,"内墙裙(m2)\n(L外内-洞口)*裙高",28,"内墙裙(m2)\n(L内-洞口)*裙高*2",null,null,44,"外墙裙(m2)\n(L外-洞口)*裙高",null,null,54,"楼地面垫层、隔热层(m3)\n52*层厚"]
[null,null,"W","汇总、复核整理",null,null,16,"外墙内面面层(m2)\nL外内*(层净高-内墙裙)*Z-Ⅰ+山尖面",29,"内墙面层(m2)\n[L内*(层净高-内墙裙)*Z-Ⅰ]*2+\n山尖面",null,null,45,"外墙面层(m2)\nL外*面层高-Ⅰ+山尖面",null,null,55,"板下勾缝(m2)\n47+52"]
[null,null,"Z","表示建筑层数",null,null,17,"外墙内面刷浆(m2)\n同16",30,"内墙刷浆(m2)\n同29",{"$nulls":6},56,"板下抹灰及刷胶(m2)\n47+52+梁侧"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet1 (2)","index":3,"n_rows":24,"n_cols":20,"rows_kept":24,"flags":["formulas_cached_only"]}
[]
[{"$nulls":12},45,"外墙面层(m2)\nL外*面层高-Ⅰ+山尖面"]
[{"$nulls":12},44,"外墙勾缝(m2)\nL外*勾缝高-Ⅰ-其他抹灰面"]
[{"$nulls":4},5,"基础防潮层(m2)\nL中*潮宽",null,null,18,"基础防潮层(m2)\nL内*潮宽",null,null,43,"外墙脚手架(m2)\nL外*砌筑高"]
[{"$nulls":4},4,"基础体积(m3)\nL中*断面面积",6,"捣制砼地梁(m3)        模板(m2)\nL中*断面面积            L中*高*2   ",19,"捣制砼地梁(m3)      模板(m2)\nL内*断面面积          L内*高*2   ",null,null,42,"散水(m2)\n(L外+坡宽*4-台阶)*坡宽"]
[{"$nulls":4},3,"基础垫层(m3)\nL中*断面面积 ",7,"捣制砼圈梁(m3)        模板(m2)\nL中*断面面积            L中*高*2   ",20,"捣制砼圈梁(m3)      模板(m2)\nL内*断面面积          L内*高*2   ",null,null,41,"砼天沟挑檐面层(m2)\n(L外+檐宽*4)*檐宽"]
[{"$nulls":4},2,"槽底夯实(m2)\nL中*槽底宽",8,"外墙身体积(m3)\n(L中*层高*Z-Ⅰ)*墙厚-Ⅱ+山尖 ",21,"内墙体积(m3)\n(L内*墙高*Z-Ⅰ)*墙厚-Ⅱ+山尖",null,null,40,"圈梁露面面层(m2)\nL外*露面高*道"]
[{"$nulls":4},1,"地槽挖土(m3)\nL中*地槽断面",9,"女儿墙体积(m3)\nL中*墙高*墙厚-Ⅱ ",22,"内墙脚手架(m2)\nL内*墙高*Z",null,null,39,"腰线面层(m2)\n(L外-洞口)*展宽*道"]
[{"$nulls":6},10,"地槽回填土(m3)\n1-∑基础体积及垫层(室外地坪下部分)",23,"内墙勾缝(m2)\n同29",null,null,38,"外墙裙(m2)\n(L外-洞口)*裙高"]
[{"$nulls":6},11,"余土外运(m3)\n1-10-51-50*系数",24,"间壁墙(m2)\n间壁长*高-洞口",null,null,37,"勒脚(m2)\n(L外-洞口)*勒脚高"]
[{"$nulls":4},"Ⅲ","L中:外墙中心线(m)\n图示尺寸","Ⅳ","L外内:外墙内净长线(m)\nL中-外墙厚*4-墙厚*道","Ⅴ","L内:内墙净长线(m)\n(图示尺寸)","Ⅵ","L内轴:内墙轴线长(m)(图示尺寸)\nL内+两端1/2墙厚","Ⅶ","L外:外墙外边线(m) \n图示尺寸或L中+墙厚*4","Ⅷ","F:底层建筑面积(m2)\n图示尺寸","Ⅹ","F楼:底层建筑面积(m2)\n图示尺寸","Ⅻ","面、线外项目按图计"]
[{"$nulls":6},12,"墙身防潮层(m2)\nL外内*潮高",25,"墙身防潮层(m2)\nL内*潮高*2",31,"地槽挖土(m3)\n(L内轴-两侧基底宽/2)*地槽断面积",null,null,"Ⅸ","F净:底层净面积(m2)\n(-L中*墙厚-L内*墙厚","Ⅺ","F楼净:底层净面积(m2)\n(-L中*墙厚-L内*墙厚","ⅫⅠ","其他项目按图或有关资料计算"]
[{"$nulls":6},13,"顶棚装饰线(m) \nL外内",26,"顶棚装饰线(m)\n(L内+梁长)*2",32,"槽底夯实(m2)\n(L内轴-两侧基底宽/2)*基底宽",null,null,46,"场地平整(m2)\nF+2*L外+16",52,"楼面面层(m2)\nFn楼净","ⅫⅡ","完成计算"]
[{"$nulls":6},14,"踢脚线(m) \n同13",27,"踢脚线(m)\nL内*2",33,"基础垫层(m3)\n(L内轴-两侧垫层宽/2)*垫层断面积",null,null,47,"地面面层(m2)  地面找平层(m2)\nF净           F净",53,"楼地面找平层、防潮层(m2)\n同52","W","汇总、复核整理"]
[{"$nulls":6},15,"内墙裙(m2)\n(L外内-洞口)*裙高",28,"内墙裙(m2)\n(L内-洞口)*裙高*2",34,"基础体积(m3)\n(L内轴-两侧基础宽/2)*基础断面积",null,null,48,"地面防潮层\n同47",54,"楼地面垫层、隔热层(m3)\n52*层厚","Z","表示建筑层数"]
[null,null,"Ⅰ","门窗表\n图示量",null,null,16,"外墙内面面层(m2)\nL外内*(层净高-内墙裙)*Z-Ⅰ+山尖面",29,"内墙面层(m2)\n[L内*(层净高-内墙裙)*Z-Ⅰ]*2+山尖面",35,"地槽回填土(m3)\n31-基础体积及垫层(室外地坪下部分)",null,null,49,"地面垫层(m3)   地面隔热层(m3)\n47*层厚        47*层厚",55,"板下勾缝(m2)\n47+52"]
[{"$nulls":6},17,"外墙内面刷浆(m2)\n同16",30,"内墙刷浆(m2)\n同29",36,"余土外运(m3)\n31-35-51",null,null,50,"地面灰土(m3)\n47*灰土厚",56,"板下抹灰及刷胶(m2)\n47+52+梁侧"]
["Y","设计资料\n熟悉图纸",{"$nulls":12},51,"地面填土(m3)\n47*填土厚",57,"满堂脚手架(m2)\n47+52"]
[null,null,"Ⅱ","墙体内埋件\n表图示量",{"$nulls":12},58,"龙骨吊顶(m2)\n47+52"]
[{"$nulls":16},59,"瓦屋面(m2)\n(F楼+外挑)*系数"]
[{"$nulls":16},60,"平屋面找平层(m2)\nF楼+41"]
[{"$nulls":16},61,"带女儿墙屋顶保温层上找平(m2)\nF楼-L中*女儿墙厚)"]
[{"$nulls":16},62,"带女儿墙屋顶保温层(m3)\n61*保温均厚"]
[{"$nulls":16},63,"带女儿墙屋面防水层(m2)\n61+(L中-女儿墙厚*4)*0.25"]

{"sheet":"Sheet1 (3)","index":4,"n_rows":15,"n_cols":18,"rows_kept":15,"merged":[[0,0,0,17]],"flags":["formulas_cached_only"]}
["建筑工程量计算程序统筹表"]
[{"$nulls":6},11,"余土外运(m3)\n  1  -  10  -  51  -  50 *系数",24,"间壁墙(m2)\n间壁长*高-洞口",36,"余土外运(m3)\n  31  -  35  -  51",{"$nulls":4},57,"板下抹灰及刷胶(m2)\n  47  +  52  +梁侧"]
[{"$nulls":6},10,"地槽回填土(m3)\n  1  -∑基础体积及垫层(室外地坪\n以下部分)",23,"内墙勾缝(m2)\n同  29",35,"地槽回填土(m3)\n  31  -基础体积及垫层(室外地坪\n下部分)",42,"外墙勾缝(m2)\nL外*勾缝高- Ⅰ -其他抹灰面",51,"地面填土(m3)\n  47  *填土厚",56,"板下勾缝(m2)\n  47  +  52"]
[{"$nulls":6},9,"女儿墙体积(m3)\nL中*墙高*墙厚-  Ⅱ ",22,"内墙脚手架(m2)\nL内*墙高*  Z",null,null,41,"外墙脚手架(m2)\nL外*砌筑高",50,"地面灰土(m3)\n  47  *灰土厚",55,"满堂脚手架(m2)\n  47  +  52"]
[{"$nulls":4},4,"基础体积(m3)\nL中*断面面积",8,"外墙体积(m3)\n(L中*层高*  Z  - Ⅰ )*墙厚-  Ⅱ\n+山尖 ",21,"内墙体积(m3)\n(L内*墙高*  Z  - Ⅰ  )*墙厚-  Ⅱ  +山尖",34,"基础体积(m3)\n(L内轴-两侧基础宽/2)*基础断面积",40,"圈梁露面面层(m2)\nL外*露面高*道",49,"地面垫层(m3)   地面隔热层(m3)\n  47  *层厚           47  *层厚",54,"楼地面垫层、隔热层(m3)\n  52  *层厚"]
[{"$nulls":4},3,"基础垫层(m3)\nL中*断面面积 ",7,"捣制砼圈梁(m3)        模板(m2)\nL中*断面面积            L中*高*2   ",20,"捣制砼圈梁(m3)      模板(m2)\nL内*断面面积          L内*高*2   ",33,"基础垫层(m3)\n(L内轴-两侧垫层宽/2)*垫层断面积",39,"腰线面层(m2)\n(L外-洞口)*展宽*道",48,"地面防潮层\n同  47",53,"楼地面找平层、防潮层(m2)\n同  52"]
[{"$nulls":4},2,"槽底夯实(m2)\nL中*槽底宽",6,"捣制砼地梁(m3)        模板(m2)\nL中*断面面积            L中*高*2   ",19,"捣制砼地梁(m3)      模板(m2)\nL内*断面面积          L内*高*2   ",32,"槽底夯实(m2)\n(L内轴-两侧基底宽/2)*基底宽",38,"散水(m2)\n(L外+坡宽*4-台阶)*坡宽",47,"地面面层(m2)  地面找平层(m2)\nF净                    F净",52,"楼面面层(m2)\nFn楼净"]
[null,null,"Ⅱ","墙体内埋件\n表图示量",1,"地槽挖土(m3)\nL中*地槽断面",5,"基础防潮层(m2)\nL中*潮宽",18,"基础防潮层(m2)\nL内*潮宽",31,"地槽挖土(m3)\n(L内轴-两侧基底宽/2)*地槽断面积",37,"砼天沟挑檐面层(m2)\n(L外+檐宽*4)*檐宽","Ⅸ","F净:底层净面积(m2)\nF-L中*墙厚-L内*墙厚","Ⅺ","F楼净:底层净面积(m2)\nF楼-L中*墙厚-L内*墙厚"]
["Y","设计资料\n熟悉图纸","Ⅰ","门窗表\n图示量","Ⅲ","L中:外墙中心线(m)\n图示尺寸","Ⅳ","L外内:外墙内净长线(m)\nL中-外墙厚*4-墙厚*道","Ⅴ","L内:内墙净长线(m)\n图示尺寸","Ⅵ","L内轴:内墙轴线长(m)\n图示尺寸或L内+两端1/2墙厚","Ⅶ","L外:外墙外边线(m) \n图示尺寸或L中+墙厚*4","Ⅷ","F:底层建筑面积(m2)\n图示尺寸","Ⅹ","F楼:楼层建筑面积(m2)\n图示尺寸"]
[{"$nulls":6},12,"墙身防潮层(m2)\nL外内*潮高",25,"墙身防潮层(m2)\nL内*潮高*2",{"$nulls":4},46,"平整场地(m2)\nF+2*L外+ 16m2",58,"龙骨吊顶(m2)\n  47  +  52"]
[null,null,"Ⅻ","面、线外项目按图计",null,null,13,"顶棚装饰线(m) \nL外内",26,"顶棚装饰线(m)\n(L内+梁长)*2",{"$nulls":6},59,"瓦屋面(m2)\n(F楼+外挑)*系数"]
[null,null,"ⅫⅠ","其他项目按图或有关资料计算",null,null,14,"踢脚线(m) \n同  13",27,"踢脚线(m)\nL内*2",null,null,43,"勒脚(m2)\n(L外-洞口)*勒脚高",null,null,60,"平屋面找平层(m2)\nF楼+  37"]
[null,null,"ⅫⅡ","完成计算",null,null,15,"内墙裙(m2)\n(L外内-洞口)*裙高",28,"内墙裙(m2)\n(L内-洞口)*裙高*2",null,null,44,"外墙裙(m2)\n(L外-洞口)*裙高",null,null,61,"带女儿墙屋顶保温层上找平(m2)\nF楼-L中*女儿墙厚"]
[null,null,"W","汇总、复核整理",null,null,16,"外墙内面面层(m2)\nL外内*(层净高-内墙裙)*  Z  - Ⅰ\n+山尖面",29,"内墙面层(m2)\n[ L内*(层净高-内墙裙)*  Z  - Ⅰ  ]\n*2+山尖面",null,null,45,"外墙面层(m2)\nL外*面层高-  Ⅰ  +山尖面",null,null,62,"带女儿墙屋顶保温层(m3)\n  61  *保温均厚"]
[null,null,"Z","表示建筑层数",null,null,17,"外墙内面刷浆(m2)\n同  16",30,"内墙刷浆(m2)\n同  29",{"$nulls":6},63,"带女儿墙屋面防水层(m2)\n  61  +(L中-女儿墙厚*4)*0.25"]