{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet1","Sheet2"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":31,"n_cols":12,"rows_kept":31,"merged":[[0,2,0,5]],"flags":["formulas_cached_only"]}
[null,null,"计算工程量简易流程图"]
["I外墙中心线"]
["L中图示尺寸"]
[]
[null,"1.基槽挖土","2.基础垫层","3.基体","4.钢筋混凝土地梁及防水圈梁","5.基础防潮层","6.钢筋混凝土圈梁","10.外墙身","11.女儿墙","12.内墙裙","13.内墙里粉刷",14]
[null,"L中+L内 *断面","同左","同左","L中+L内 *梁断面","L中+L内 *B","L中*梁断面*道","[L中*H—V]*B-VI","L中*H*B","L中*H*Z","L中*H*Z-12-V"]
[]
[]
[]
["II 内墙净长线",null,"7.回填土",null,"8.余土外运","9.钢筋混凝土圈梁","14.内墙身","15.间壁墙","16.墙裙","17.内墙面粉刷",18]
["L内图示尺寸",null,"1~2~6",null,"1~7","L内*梁断面*道","[L内*H—V]*B-VI","L内*H—V","L内*H*2*Z","L内*H*2*Z—16—V"]
[]
[]
[]
["III 外墙外边线","18.勒脚","19腰线面层","20.外墙面层","21.混凝土天沟挑檐面层","22.明沟","23.散水","24.外墙脚手架",25]
["L外图示尺寸","L外*H","L外*H","L外*H—V","L外*展开面宽","L外","L外*B","L外*H"]
[]
[]
[]
["IV底层建筑面积","25.场地平整","26.室内围土","27.地坪垫层","28.地坪面层","29.楼面面层","30.钢筋混凝土楼板","31.吊平顶","32.平顶粉刷","33.综合脚本架","34.屋面找平层","35.屋面防水层"]
["S1","S1+2L外+16","[S1—5]*H","同左","S1—5","S1—Z","29*H","同28","同28","S1*Z","S1+21","34弯起部分"]
[{"$nulls":11},36]
[]
[]
["V 门窗数量表"]
["图示数量"]
[]
[]
[]
["VI 墙体埋件表"]
["按图计算"]

{"sheet":"Sheet2","index":1,"n_rows":30,"n_cols":6,"rows_kept":30,"merged":[[0,0,0,5],[24,2,24,4]],"flags":["formulas_cached_only"]}
["计算工程量简易流程图"]
["I外墙中心线"]
["L中图示尺寸"]
[null,"1.基槽挖土(m3)","2.基础垫层(m3)","3.基体(m3)","4.钢筋砼地梁及防水圈梁(m3)","5.基础防潮层(m2)"]
[null,"L中+L内 *断面","同左","同左","L中+L内 *梁断面","L中+L内 *B           6"]
[]
[null,"6.钢筋混凝土圈梁(m3)","10.外墙身(m3)","11.女儿墙(m3)","12.内墙裙(m2)","13.外墙里粉刷(m2)"]
[null,"L中*梁断面*道","[L中*H—V]*B-VI","L中*H*B","L中*H*Z","L中*H*Z-12-V      14        "]
[]
["II 内墙净长线","7.回填土(m3)","8.余土外运(m3)","9.钢筋砼圈梁(m3)","14.内墙身(m3)","15.间壁墙(m2)"]
["L内图示尺寸","1~2~6","1~7","L内*梁断面*道","[L内*H—V]*B-VI","L内*H—V"]
[{"$nulls":3},"16.墙裙(m2)","17.内墙面粉刷(m2)"]
[{"$nulls":3},"L内*H*2*Z","L内*H*2*Z—16—V                18"]
[]
["III 外墙外边线（M）","18.勒脚(m2.)","19腰线面层(m2)","20.外墙面层(m2)","21.砼天沟挑檐面层(m2)","22.明沟(m)"]
["L外图示尺寸","L外*H","L外*H","L外*H—V","L外*展开面宽","L外                    23"]
[{"$nulls":3},"23.散水(m2)","24.外墙脚手架(m3)",25]
[{"$nulls":3},"L外*B","L外*H"]
[]
["IV底层建筑面积(m2)","25.场地平整(m2)","26.室内围土(m3)","27.地坪垫层(m3)","28.地坪面层(m2)","29.楼面面层(m2)"]
["S1","S1+2L外+16","[S1—5]*H","同左","S1—5","S1—Z                 30"]
[]
["30.钢筋砼楼板(m2)","31.吊平顶(m2)","32.平顶粉刷(m2)","33.综合脚本架(m2)","34.屋面找平层(m2)","35.屋面防水层(m2)"]
["29*H","同28","同28","S1*Z","S1+21","34弯起部分         36"]
[null,null,"图                                                               例"]
["V 门窗数量表",null,"L中  ——外墙中心线","                     流程线","Y   ——熟悉设计资料"]
["图示数量",null,"L外  ——外墙外边线","B        ——墙的厚度","Ⅰ  ——分项计算顺序"]
[null,null,"Z     ——建筑物层数","L内 ——内墙净长线","H   ——层高（高度）"]
["VI 墙体埋件表",null,"⑴ ——基数计算程序","S1 ——底层建筑面积"]
["按图计算"]