{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":1,"external_links":1,"comments":50},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":58,"n_cols":15,"rows_kept":58,"merged":[[0,0,1,3],[0,4,0,8],[0,9,0,10],[0,11,0,13],[1,4,1,8],[1,9,1,10],[1,11,1,12],[1,13,1,14],[2,0,2,3],[2,4,2,8],[2,9,2,10],[2,11,2,14],[3,0,8,0],[3,1,8,1],[3,2,4,2],[3,3,4,4],[3,5,4,8],[3,9,4,10],[3,11,4,13],[5,3,5,8],[5,9,5,13],[6,3,6,8],[6,9,6,13],[7,3,7,4],[7,5,7,8],[7,9,7,10],[7,11,7,13],[8,3,8,8],[8,9,8,10],[8,11,8,13],[9,0,19,0],[9,1,19,1],[9,3,9,4],[9,5,9,8],[9,9,9,10],[9,11,9,13],[10,2,11,2],[10,3,10,8],[10,10,10,11],[10,12,10,13],[11,3,11,8],[11,10,11,11],[11,12,11,13],[12,3,12,8],[12,9,12,13],[13,3,13,8],[13,9,13,13],[14,3,14,8],[14,9,14,13],[15,3,15,4],[15,5,15,8],[15,9,15,10],[15,11,15,13],[16,3,16,4],[16,5,16,8],[16,9,16,10],[16,11,16,13],[17,3,17,8],[17,9,17,13],[18,3,18,8],[18,9,18,13],[19,3,19,8],[19,9,19,13],[20,0,30,0],[20,1,30,1],[20,3,20,8],[20,9,20,13],[21,3,21,8],[21,9,21,13],[22,3,22,8],[22,9,22,13],[23,3,23,4],[23,5,23,8],[23,9,23,10],[23,11,23,13],[24,3,24,8],[24,9,24,13],[25,3,25,4],[25,5,25,8],[25,9,25,10],[25,11,25,13],[26,3,26,8],[26,9,26,13],[27,3,27,8],[27,9,27,13],[28,3,28,4],[28,5,28,8],[28,9,28,10],[28,11,28,13],[29,3,29,8],[29,9,29,13],[30,3,30,8],[30,9,30,13],[31,0,40,0],[31,1,40,1],[31,3,31,8],[31,9,31,13],[32,3,32,8],[32,9,32,13],[33,3,33,8],[33,9,33,13],[34,3,34,8],[34,9,34,13],[35,3,35,8],[35,9,35,13],[36,3,36,8],[36,9,36,13],[37,3,37,8],[37,9,37,13],[38,3,38,8],[38,9,38,13],[39,3,39,8],[39,9,39,13],[40,3,40,8],[40,9,40,13],[41,0,44,0],[41,1,44,1],[41,3,41,8],[41,9,41,13],[42,3,42,8],[42,9,42,13],[43,3,43,8],[43,9,43,13],[44,3,44,8],[44,9,44,13],[45,0,48,0],[45,1,48,1],[45,3,45,8],[45,9,45,13],[46,3,46,8],[46,9,46,13],[47,3,47,8],[47,9,47,13],[48,3,48,8],[48,9,48,13],[49,0,49,14],[50,0,56,14],[57,0,57,3],[57,4,57,7],[57,8,57,9],[57,10,57,14]],"flags":["formulas_cached_only"]}
[{"$nulls":4},"仪表规格书（自力式调节阀）",{"$nulls":4},"档案号PROJECT No："]
[{"$nulls":4},"INSTRUMENT SPECIFICATION",{"$nulls":4},"设计阶段 STAGE：",{"$nulls":3},"版本  FA"]
[{"$nulls":4},"(REGULATOR)",{"$nulls":4},"页数PAGE："]
["概况","General",1,"位号 Tag Number",null,"数量 Quantity",{"$nulls":8},"REV"]
[]
[null,null,2,"检测位置 Service"]
[null,null,3,"P&ID Number"]
[null,null,4,"工艺管道尺寸Pipe Size",null,"等级 Class"]
[null,null,5,"工艺管道材质 Piping Mat'l"]
["操作条件","Operating Conditions",6,"介质名称 Fluid",null,"状态  State"]
[null,null,7,"流量 Flow  Rate",{"$nulls":5},"最大MaxFlow","正常 NorFlow",null,"最小MinFlow"]
[{"$nulls":3}," kg/h(液体Liquid,蒸汽Steam）Nm3/h(气体Gas)"]
[null,null,8,"阀前压力 Inlet Pressure MPa(G)"]
[null,null,9,"阀后压力 Outlet Pressure MPa(G)"]
[null,null,10,"操作温度 Oper Temp( ℃ )"]
[null,null,11,"操作密度Oper. Density kg/m3",null,"标准密度Std. Density kg/m3n"]
[null,null,12,"运动粘度 Kin Visc(mm2/S)",null,"动力粘度 Dyn Visc(mPa.s)"]
[null,null,13,"摩尔分子量 Molecular WT"]
[null,null,14]
[null,null,15]
["阀体","Valve Body",16,"名称 Name"]
[null,null,17,"型号  Model"]
[null,null,18,"型式 Type"]
[null,null,19,"公称通径 Body Size",null,"公称压力 Rating Pre(MPa)"]
[null,null,20,"流量特性 Charact"]
[null,null,21,"计算Cv值 Sizing Cv",null,"额定Cv值 Rated  Cv"]
[null,null,22,"阀门连接型式和标准 End Conn. Style & Std."]
[null,null,23,"阀体材质及阀盖材质      Body/Bonnet MAT’L",null,"阀芯材质 Trim Mat'l"]
[null,null,24,"阀芯材质 Trim Mat'l",null,"填料材质  Packing MAT'L"]
[null,null,25]
[null,null,26]
["执行机构","Actuator",27,"型号  Model"]
[null,null,28,"膜头允许压差 Allowed Different Pressure of Diaphragm "]
[null,null,29,"压力平衡元件 Pressure Balance Component"]
[null,null,30,"膜片材质  Diaphragm Mat'l"]
[null,null,31,"弹簧材质  Spring Mat'l"]
[null,null,32,"设定压力  Setting Press."]
[null,null,33,"调压范围  Calibration Range"]
[null,null,34,"精度 Accuracy"]
[null,null,35]
[null,null,36]
["附件","Accessories",37,"信号阀  Pilot Valve"]
[null,null,38]
[null,null,39]
[null,null,40]
["其他","Miscell.",41,"制造商 Manufacturer"]
[null,null,42]
[null,null,43]
[null,null,44]
["说明 NOTES："]
{"$rows_empty":7}
["编制",{"$nulls":3},"校对",{"$nulls":3},"审核",null,"日期"]