{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":69,"rows_kept":14,"flags":["formulas_cached_only"]}
[{"$nulls":3},"单阶柱稳定","性计算","长度单位:","mm","力单位:","N","Nmm","应力单位：","Mpa"]
[{"$nulls":5},"输入端弯矩时应注意：Mx2的绝对值 大于Mx1的绝对值"]
[{"$nulls":7},"若Mx2和Mx1反号，Mx1取负值"]
["几何条件","上柱","截面信息",{"$nulls":11},"柱长度","荷载",{"$nulls":3},"下柱","截面信息",{"$nulls":11},"柱长度","荷载",{"$nulls":3},"材料性质",{"$nulls":3},"求计算长度系数",{"$nulls":3},"计算长度系数",null,null,"下柱平面内稳定",{"$nulls":11},"下柱平面外稳定"]
[null,"请输入：","截面高度","翼缘宽度","腹板厚度","翼缘厚度","自动计算：","面积","强轴惯性矩","强轴抵抗矩","弱轴惯性矩","回转半径","回转半径","请输入：","柱长度","轴力","柱端弯矩1","柱端弯矩2",null,"请输入：","截面高度","翼缘宽度","腹板厚度","翼缘厚度","自动计算：","面积","强轴惯性矩","强轴抵抗矩","弱轴惯性矩","回转半径","回转半径","请输入：","柱长度","轴力","柱端弯矩1","柱端弯矩2","请输入：","弹性模量","强度","屈服强度","自动计算：",null," ",null,"请根据","下柱（查表）","上柱(自动计算）",null,null,"自动计算","(根据λx查表）",null,"请输入","（根据柱端弯矩查表）",null,null,"自动计算",null,"自动计算",null,null,"自动计算","(根据λy查表）",null,"自动计算","（根据柱端弯矩查表）",null,null,"自动计算"]
[null,null,"H","b","tf","tw",null,"A","Ix","Wx","Iy"," 小Ix"," 小Iy",null,"H1","N1","M11","M12",null,null,"H","b","tf","tw",null,"A","Ix","Wx","Iy"," 小Ix"," 小Iy",null,"H2","N2","M21","M22",null,"E","f","fy"," ",null," η1 ","K1","η1K1查表","u2请输入","u1自动计算",null,null,"λx",null,"φx   ","γx ",null,"βmx",null,"NEX",null,"应力",null,null,"λy",null,"φy   ","φb   ",null,"βtx",null,"应力"]
[null,null,700,250,10,12,null,12760,967517813.333333,2764336.6095238086,31306333.333333332,275.36208896977314,49.53255898057412,null,6320,49815,{"v":-86332000,"d":"-8.63E+07"},{"v":317240000,"d":"3.17E+08"},null,null,1200,500,10,18,null,29640,7601793120,12669655.2,375097000,506.4294156508262,112.49486418026635,null,9530,{"v":1861000,"d":"1.86E+06"},{"v":1133700000,"d":"1.13E+09"},{"v":1362200000,"d":"1.36E+09"},null,{"v":206000,"d":"2.06E+05"},200,235,null,null,{"v":0.3041302344067354,"d":"3.04E-01"},0.1919193419302324,"注意梁柱",1.875,{"v":6.165122003267937,"d":"6.17E+00"},null,null,35.28379167516639,null,0.92,1.05,null,1,null,{"v":48405493.458997205,"d":"4.84E+07"},null,{"v":173.89273198912127,"d":"1.74E+02"},null,null,84.71497849651821,null,0.657,0.9085258794125253,null,{"v":0.941289825282631,"d":"9.41E-01"},null,{"v":206.95995486407048,"d":"2.07E+02"}]
[{"$nulls":44},"刚结铰结"]
[]
[{"$nulls":50}," "]
[{"$nulls":48},"上柱平面内稳定",{"$nulls":11},"上柱平面外稳定"]
[{"$nulls":49},"自动计算","(根据λx查表）",null,"请输入","（根据柱端弯矩查表）",null,null,"自动计算",null,"自动计算",null,null,"自动计算","(根据λy查表）",null,"自动计算","（根据柱端弯矩查表）",null,null,"自动计算"]
[{"$nulls":49},"λx",null,"φx   ","γx ",null,"βmx",null,"NEX",null,"应力",null,null,"λy",null,"φy   ","φb   ",null,"βtx",null,"应力"]
[{"$nulls":49},{"v":141.49940250101184,"d":"1.41E+02"},null,0.341,1.05,null,1,null,{"v":1295711.7983127057,"d":"1.30E+06"},null,{"v":124.21383928489792,"d":"1.24E+02"},null,null,127.5928425680289,null,0.399,0.7000015119411408,null,{"v":0.5547528684907326,"d":"5.55E-01"},null,{"v":100.7333833584909,"d":"1.01E+02"}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}