{"text_format":"3","workbook":"xls","n_sheets":13,"sheets":["601","602","603","604","605","606","607","608","609","610","611","612","613"],"not_rendered":{"external_links":1,"defined_names":13},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"601","index":0,"n_rows":36,"n_cols":10,"rows_kept":36,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,4],[2,6,2,8],[3,0,3,4],[3,6,3,8],[4,0,4,1],[4,2,4,4],[4,6,4,7],[4,8,7,8],[5,0,5,1],[5,2,5,4],[5,6,5,7],[6,0,7,0],[6,1,7,3],[6,4,7,4],[6,5,7,7],[8,0,11,0],[8,1,11,1],[8,2,8,3],[8,5,8,7],[8,8,25,8],[9,2,9,3],[9,5,9,7],[10,2,10,3],[10,5,10,7],[11,2,11,3],[11,5,11,7],[12,0,14,0],[12,1,14,1],[12,2,12,3],[12,5,12,7],[13,2,13,3],[13,5,13,7],[14,2,14,3],[14,5,14,7],[15,0,17,0],[15,1,17,1],[15,2,15,3],[15,5,15,7],[16,2,16,3],[16,5,16,7],[17,2,17,3],[17,5,17,7],[18,1,18,3],[18,5,18,7],[19,0,22,0],[19,1,22,1],[19,2,19,3],[19,5,19,7],[20,2,20,3],[20,5,20,7],[21,2,21,3],[21,5,21,7],[22,2,22,3],[22,5,22,7],[23,1,23,3],[23,5,23,7],[24,0,25,0],[24,1,25,1],[24,2,24,3],[24,5,24,7],[25,2,25,3],[25,5,25,7],[26,0,29,8],[30,0,34,8],[35,0,40,8]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表601              路面标线检验汇总表",{"$nulls":8}," "]
["承包单位： ",{"$nulls":5},"合同号："]
["监理单位： ",{"$nulls":5},"编    号：",null,null," "]
["工 程 名 称",{"$nulls":4},"施工日期",null,null,"外观\n检测"," "]
["桩号及部位",{"$nulls":4},"检验日期",{"$nulls":3}," "]
["项次","检查项目",null,null,"规定值或\n允许偏差","检测结果",{"$nulls":3}," "]
[{"$nulls":9}," "]
[1,"标线长度（mm）",6000,null,"±50"]
[null,null,4000,null,"±40"]
[null,null,3000,null,"±30"]
[null,null,"1000-2000",null,"±20"]
[2,"标线宽度（mm）","400-500",null,"+15\n-0"]
[null,null,"150-200",null,"+8\n-0"]
[null,null,100,null,"+5\n-0"]
[3,"标线厚度（mm）","常温型（0.12-0.2）",null,"+0.1\n-0.03"]
[null,null,"加热型（0.2-0.4）",null,"+0.15\n-0.05"]
[null,null,"热熔型（1.0-4.50）",null,"+0.50\n-0.10"]
[4,"标线横向偏位（mm）",null,null,"±30"]
[5,"标线纵\n向间距（mm）",9000,null,"±45"]
[null,null,6000,null,"±30"]
[null,null,4000,null,"±20"]
[null,null,3000,null,"±15"]
[6,"标线剥落面积",null,null,"总面积的0-3%"]
[7,"反光标线逆反射系数","白色标线",null,"≥150"]
[null,null,"黄色标线",null,"≥100"]
["自检结果：\n\n\n\n技术负责人：　　　　　　日期：　　　　　　项目负责人：　　　　　　日期：",{"$nulls":8}," "]
[]
[]
[]
["监理评定：\n\n\n\n\n专业工程师：　　　　测量工程师：　　　    　试验工程师：　　　　　    日期："]
[]
[]
[]
[]
["结   论：\n\n\n\n           \n                                                                                    驻地工程师：                        日期："]

{"sheet":"602","index":1,"n_rows":32,"n_cols":10,"rows_kept":32,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,4],[2,6,2,8],[3,0,3,4],[3,6,3,8],[4,0,4,1],[4,2,4,4],[4,6,4,7],[4,8,7,8],[5,0,5,1],[5,2,5,4],[5,6,5,7],[6,0,7,0],[6,1,7,3],[6,4,7,4],[6,5,7,7],[8,1,8,3],[8,5,8,7],[8,8,12,8],[9,1,9,3],[9,5,9,7],[10,1,10,3],[10,5,10,7],[11,1,11,3],[11,5,11,7],[12,1,12,3],[12,5,12,7],[13,0,18,8],[19,0,24,8],[25,0,30,8]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表602              突起路标检验汇总表",{"$nulls":8}," "]
["承包单位： ",{"$nulls":5},"合同号："]
["监理单位： ",{"$nulls":5},"编    号：",null,null," "]
["工 程 名 称",{"$nulls":4},"施工日期",null,null,"外观\n检测"," "]
["桩号及部位",{"$nulls":4},"检验日期",{"$nulls":3}," "]
["项次","检查项目",null,null,"规定值或允许偏差","检测结果",{"$nulls":3}," "]
[{"$nulls":9}," "]
[1,"安装角度（°）",null,null,"±5",{"$nulls":4}," "]
[2,"纵向间距（mm）",null,null,"±50"]
[4,"横向偏位（mm）",null,null,"±30"]
[5,"抗压强度（KN）",null,null,"160",{"$nulls":4}," "]
[6,"损坏及脱落个数（%）",null,null,"＜0.5",{"$nulls":4}," "]
["自检结果：\n\n\n\n\n\n\n技术负责人：　　　　　　日期：　　　　　　项目负责人：　　　　　　日期：",{"$nulls":8}," "]
[]
[]
[]
[]
[]
["监理评定：\n\n\n\n\n\n\n专业工程师：　　　　测量工程师：　　　　　试验工程师：　　　　　   日期："]
[]
[]
[]
[]
[]
["结　论：　　　　　　　　　　　　　　　　　　　　\n\n\n\n\n\n　　　　　　　　　　　　　　　　　　　　　驻地工程师：            日期："]
[]
[]
[]
[]
[]
[{"$nulls":9}," "]

{"sheet":"603","index":2,"n_rows":37,"n_cols":10,"rows_kept":37,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,4],[2,6,2,8],[3,0,3,4],[3,6,3,8],[4,0,4,1],[4,2,4,4],[4,6,4,7],[4,8,7,8],[5,0,5,1],[5,2,5,4],[5,6,5,7],[6,0,7,0],[6,1,7,3],[6,4,7,4],[6,5,7,7],[8,1,8,3],[8,5,8,7],[8,8,16,8],[9,1,9,3],[9,5,9,7],[10,1,10,3],[10,5,10,7],[11,1,11,3],[11,5,11,7],[12,1,12,3],[12,5,12,7],[13,1,13,3],[13,5,13,7],[14,1,14,3],[14,5,14,7],[15,1,15,3],[15,5,15,7],[16,1,16,3],[16,5,16,7],[17,0,22,8],[23,0,29,8],[30,0,35,8]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表603               交通标志检验汇总表",{"$nulls":8}," "]
["承包单位： ",{"$nulls":5},"合同号："]
["监理单位： ",{"$nulls":5},"编    号：",null,null," "]
["工 程 名 称",{"$nulls":4},"施工日期",null,null,"外观\n检测"," "]
["桩号及部位",{"$nulls":4},"检验日期",{"$nulls":3}," "]
["项次","检查项目",null,null,"规定值或允许偏差","检测结果",{"$nulls":3}," "]
[{"$nulls":9}," "]
[1,"基础砼强度（Mpa）",null,null,"合格标\n准    内"]
[2,"标志板外形尺寸（mm）",null,null,"±5"]
[3,"标志板厚度（mm）",null,null,"不小于\n设计值"]
[4,"标志汉字、数字、拉丁字的字体及尺寸（mm）",null,null,"符合设\n计要求"]
[5,"标志面反光膜等级\n及逆反射系数",null,null,"符合\n要求",{"$nulls":4}," "]
[6,"标志板下缘至路面净空高度及标志板内缘距路面边缘距离（mm）",null,null,"100",{"$nulls":4}," "]
[7,"立柱竖直度（mm/m）",null,null,"±3"]
[8,"标志金属构件镀层厚度",null,null,"符合规\n范要求"]
[9,"标志基础尺寸（mm）",null,null,"+100\n-50"]
["自检结果：\n\n\n\n\n\n\n技术负责人：　　　　　　日期：　　　　　　项目负责人：　　　　　　日期：",{"$nulls":8}," "]
[]
[]
[]
[]
[]
["监理评定：\n\n\n\n\n\n\n\n专业工程师：　　　　测量工程师：　　　　　试验工程师：　　　　　     日期："]
[]
[]
[]
[]
[]
[]
["结　论：　　　　　　　　　　　　　　　　　　　　\n\n\n\n\n\n　　　　　　　　　　　　　　　　　　　　　驻地工程师：             日期："]
[]
[]
[]
[]
[]
[{"$nulls":9}," "]

{"sheet":"604","index":3,"n_rows":32,"n_cols":10,"rows_kept":32,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,4],[2,6,2,8],[3,0,3,4],[3,6,3,8],[4,0,4,1],[4,2,4,4],[4,6,4,7],[4,8,7,8],[5,0,5,1],[5,2,5,4],[5,6,5,7],[6,0,7,0],[6,1,7,3],[6,4,7,4],[6,5,7,7],[8,1,8,3],[8,5,8,7],[8,8,11,8],[9,1,9,3],[9,5,9,7],[10,1,10,3],[10,5,10,7],[11,1,11,3],[11,5,11,7],[12,0,17,8],[18,0,24,8],[25,0,30,8]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表604              视线诱导标检验汇总表",{"$nulls":8}," "]
["承包单位： ",{"$nulls":5},"合同号："]
["监理单位： ",{"$nulls":5},"编    号：",null,null," "]
["工 程 名 称",{"$nulls":4},"施工日期",null,null,"外观\n检测"," "]
["桩号及部位",{"$nulls":4},"检验日期",{"$nulls":3}," "]
["项次","检查项目",null,null,"规定值或允许偏差","检测结果",{"$nulls":3}," "]
[{"$nulls":9}," "]
[1,"反射器中心高度（mm）",null,null,"±35"]
[2,"反射器中距（mm）",null,null,"±100"]
[3,"反射器安装角度（°）",null,null,"±3",{"$nulls":4}," "]
[4,"反射器横向偏位",null,null,"±20",{"$nulls":4}," "]
["自检结果：\n\n\n\n\n\n\n技术负责人：　　　　　　日期：　　　　　　项目负责人：　　　　　　日期：",{"$nulls":8}," "]
[]
[]
[]
[]
[]
["监理评定：\n\n\n\n\n\n\n\n专业工程师：　　　　测量工程师：　　　　　试验工程师：　　　　    　日期："]
[]
[]
[]
[]
[]
[]
["结　论：　　　　　　　　　　　　　　　　　　　　\n\n\n\n\n\n　　　　　　　　　　　　　　　　　　　　　驻地工程师：            日期："]
[]
[]
[]
[]
[]
[{"$nulls":9}," "]

{"sheet":"605","index":4,"n_rows":33,"n_cols":10,"rows_kept":33,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,4],[2,6,2,8],[3,0,3,4],[3,6,3,8],[4,0,4,1],[4,2,4,4],[4,6,4,7],[4,8,7,8],[5,0,5,1],[5,2,5,4],[5,6,5,7],[6,0,7,0],[6,1,7,3],[6,4,7,4],[6,5,7,7],[8,1,8,3],[8,5,8,7],[8,8,12,8],[9,1,9,3],[9,5,9,7],[10,1,10,3],[10,5,10,7],[11,1,11,3],[11,5,11,7],[12,1,12,3],[12,5,12,7],[13,0,18,8],[19,0,25,8],[26,0,31,8]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表605             波形梁护栏检验汇总表",{"$nulls":8}," "]
["承包单位： ",{"$nulls":5},"合同号："]
["监理单位： ",{"$nulls":5},"编    号：",null,null," "]
["工 程 名 称",{"$nulls":4},"施工日期",null,null,"外观\n检测"," "]
["桩号及部位",{"$nulls":4},"检验日期",{"$nulls":3}," "]
["项次","检查项目",null,null,"规定值或允许偏差","检测结果",{"$nulls":3}," "]
[{"$nulls":9}," "]
[1,"横梁中心高度（mm）",null,null,"±20"]
[2,"立柱外边缘距路肩边线距离（mm）",null,null,"±20"]
[3,"立柱中距（mm）",null,null,"±5",{"$nulls":4}," "]
[4,"立柱竖直度（mm）",null,null,"±5",{"$nulls":4}," "]
[5,"护栏顺直度（mm）",null,null,"±5"]
["自检结果：\n\n\n\n\n\n\n技术负责人：　　　　　　日期：　　　　　　项目负责人：　　　　　　日期：",{"$nulls":8}," "]
[]
[]
[]
[]
[]
["监理评定：\n\n\n\n\n\n\n\n专业工程师：　　　　测量工程师：　　　　　试验工程师：　　　　    　日期："]
[]
[]
[]
[]
[]
[]
["结　论：　　　　　　　　　　　　　　　　　　　　\n\n\n\n\n\n　　　　　　　　　　　　　　　　　　　　　驻地工程师：            日期："]
[]
[]
[]
[]
[]
[{"$nulls":9}," "]

{"sheet":"606","index":5,"n_rows":32,"n_cols":10,"rows_kept":32,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,4],[2,6,2,8],[3,0,3,4],[3,6,3,8],[4,0,4,1],[4,2,4,4],[4,6,4,7],[4,8,7,8],[5,0,5,1],[5,2,5,4],[5,6,5,7],[6,0,7,0],[6,1,7,3],[6,4,7,4],[6,5,7,7],[8,1,8,3],[8,5,8,7],[8,8,11,8],[9,1,9,3],[9,5,9,7],[10,1,10,3],[10,5,10,7],[11,1,11,3],[11,5,11,7],[12,0,17,8],[18,0,24,8],[25,0,30,8]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表606              防眩设施检验汇总表",{"$nulls":8}," "]
["承包单位： ",{"$nulls":5},"合同号："]
["监理单位： ",{"$nulls":5},"编    号：",null,null," "]
["工 程 名 称",{"$nulls":4},"施工日期",null,null,"外观\n检测"," "]
["桩号及部位",{"$nulls":4},"检验日期",{"$nulls":3}," "]
["项次","检查项目",null,null,"规定值或允许偏差","检测结果",{"$nulls":3}," "]
[{"$nulls":9}," "]
[1,"板条设置间距（mm）",null,null,"±50",{"$nulls":4}," "]
[2,"竖直度（mm/m）",null,null,"±5"]
[3,"防眩高度（mm）",null,null,"±10"]
[4,"顺直度（mm/m）",null,null,"8",{"$nulls":4}," "]
["自检结果：\n\n\n\n\n\n\n技术负责人：　　　　　　日期：　　　　　　项目负责人：　　　　　　日期：",{"$nulls":8}," "]
[]
[]
[]
[]
[]
["监理评定：\n\n\n\n\n\n\n\n专业工程师：　　　　测量工程师：　　　　　试验工程师：　　　　　     日期："]
[]
[]
[]
[]
[]
[]
["结　论：　　　　　　　　　　　　　　　　　　　　\n\n\n\n\n\n　　　　　　　　　　　　　　　　　　　　　驻地工程师：             日期："]
[]
[]
[]
[]
[]
[{"$nulls":9}," "]

{"sheet":"607","index":6,"n_rows":35,"n_cols":10,"rows_kept":35,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,4],[2,6,2,8],[3,0,3,4],[3,6,3,8],[4,0,4,1],[4,2,4,4],[4,6,4,7],[4,8,7,8],[5,0,5,1],[5,2,5,4],[5,6,5,7],[6,0,7,0],[6,1,7,3],[6,4,7,4],[6,5,7,7],[8,1,8,3],[8,5,8,7],[8,8,14,8],[9,1,9,3],[9,5,9,7],[10,1,10,3],[10,5,10,7],[11,1,11,3],[11,5,11,7],[12,1,12,3],[12,5,12,7],[13,1,13,3],[13,5,13,7],[14,1,14,3],[14,5,14,7],[15,0,20,8],[21,0,27,8],[28,0,33,8]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表607            隔离栅、防落网检验汇总表",{"$nulls":8}," "]
["承包单位： ",{"$nulls":5},"合同号："]
["监理单位： ",{"$nulls":5},"编    号：",null,null," "]
["工 程 名 称",{"$nulls":4},"施工日期",null,null,"外观\n检测"," "]
["桩号及部位",{"$nulls":4},"检验日期",{"$nulls":3}," "]
["项次","检查项目",null,null,"规定值或允许偏差","检测结果",{"$nulls":3}," "]
[{"$nulls":9}," "]
[1,"砼强度（Mpa）",null,null,"合格标\n准   内"]
[2,"高度（mm）",null,null,"±15"]
[3,"镀（涂）层厚度（mm）",null,null,"符合设\n计要求"]
[4,"网面平整度",null,null,"±2",{"$nulls":4}," "]
[5,"立柱中距（mm）",null,null,"±30",{"$nulls":4}," "]
[6,"立柱埋深（mm）",null,null,"符合设\n计要求"]
[7,"立柱竖直度（mm）",null,null,"±8"]
["自检结果：\n\n\n\n\n\n\n技术负责人：　　　　　　日期：　　　　　　项目负责人：　　　　　　日期：",{"$nulls":8}," "]
[]
[]
[]
[]
[]
["监理评定：\n\n\n\n\n\n\n\n专业工程师：　　　　测量工程师：　　　　　试验工程师：　　　　　    日期："]
[]
[]
[]
[]
[]
[]
["结　论：　　　　　　　　　　　　　　　　　　　　\n\n\n\n\n\n　　　　　　　　　　　　　　　　　　　　　驻地工程师：            日期："]
[]
[]
[]
[]
[]
[{"$nulls":9}," "]

{"sheet":"608","index":7,"n_rows":32,"n_cols":10,"rows_kept":32,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,4],[2,6,2,8],[3,0,3,4],[3,6,3,8],[4,0,4,1],[4,2,4,4],[4,6,4,7],[4,8,7,8],[5,0,5,1],[5,2,5,4],[5,6,5,7],[6,0,7,0],[6,1,7,3],[6,4,7,4],[6,5,7,7],[8,1,8,3],[8,5,8,7],[8,8,11,8],[9,1,9,3],[9,5,9,7],[10,1,10,3],[10,5,10,7],[11,1,11,3],[11,5,11,7],[12,0,17,8],[18,0,24,8],[25,0,30,8]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表608               轮廓标检验汇总表",{"$nulls":8}," "]
["承包单位： ",{"$nulls":5},"合同号："]
["监理单位： ",{"$nulls":5},"编    号：",null,null," "]
["工 程 名 称",{"$nulls":4},"施工日期",null,null,"外观\n检测"," "]
["桩号及部位",{"$nulls":4},"检验日期",{"$nulls":3}," "]
["项次","检查项目",null,null,"规定值或允许偏差","检测结果",{"$nulls":3}," "]
[{"$nulls":9}," "]
[1,"安装角度（°）",null,null,"0-5",{"$nulls":4}," "]
[2,"反射器高度（mm）",null,null,"±20"]
[3,"反射器安装尺寸（mm）",null,null,"±5"]
[4,"反射器外形尺寸（mm）",null,null,"±5",{"$nulls":4}," "]
["自检结果：\n\n\n\n\n\n\n技术负责人：　　　　　　日期：　　　　　　项目负责人：　　　　　　日期：",{"$nulls":8}," "]
[]
[]
[]
[]
[]
["监理评定：\n\n\n\n\n\n\n\n专业工程师：　　　　测量工程师：　　　　　试验工程师：　　　　　     日期："]
[]
[]
[]
[]
[]
[]
["结　论：　　　　　　　　　　　　　　　　　　　　\n\n\n\n\n\n　　　　　　　　　　　　　　　　　　　　　驻地工程师：             日期："]
[]
[]
[]
[]
[]
[{"$nulls":9}," "]

{"sheet":"609","index":8,"n_rows":34,"n_cols":10,"rows_kept":34,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,4],[2,6,2,8],[3,0,3,4],[3,6,3,8],[4,0,4,1],[4,2,4,4],[4,6,4,7],[4,8,7,8],[5,0,5,1],[5,2,5,4],[5,6,5,7],[6,0,7,0],[6,1,7,3],[6,4,7,4],[6,5,7,7],[8,1,8,3],[8,5,8,7],[8,8,13,8],[9,1,9,3],[9,5,9,7],[10,0,11,0],[10,1,11,1],[10,2,10,3],[10,5,10,7],[11,2,11,3],[11,5,11,7],[12,1,12,3],[12,5,12,7],[13,1,13,3],[13,5,13,7],[14,0,19,8],[20,0,26,8],[27,0,32,8]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表609             井（孔）砌筑检验汇总表",{"$nulls":8}," "]
["承包单位： ",{"$nulls":5},"合同号："]
["监理单位： ",{"$nulls":5},"编    号：",null,null," "]
["工 程 名 称",{"$nulls":4},"施工日期",null,null,"外观\n检测"," "]
["桩号及部位",{"$nulls":4},"检验日期",{"$nulls":3}," "]
["项次","检查项目",null,null,"规定值或允许偏差","检测结果",{"$nulls":3}," "]
[{"$nulls":9}," "]
[1,"混凝土或砂浆强度（MPa）",null,null,"在合格\n标准内",{"$nulls":4}," "]
[2,"轴线偏位（mm）",null,null,"50"]
[3,"井盖与相邻路高差（mm）","雨水井",null,"+0\n-4"]
[null,null,"检查井",null,"+4\n0"]
[4,"井底高程（mm）",null,null,"±15",{"$nulls":4}," "]
[5,"圆井直径或方井长、宽（mm）",null,null,"±20",{"$nulls":4}," "]
["自检结果：\n\n\n\n\n\n\n技术负责人：　　　　　　日期：　　　　　　项目负责人：　　　　　　日期：",{"$nulls":8}," "]
[]
[]
[]
[]
[]
["监理评定：\n\n\n\n\n\n\n\n专业工程师：　　　　测量工程师：　　         　试验工程师：　　　　　    日期："]
[]
[]
[]
[]
[]
[]
["结　论：　　　　　　　　　　　　　　　　　　　　\n\n\n\n\n\n　　　　　　　　　　　　　　　　　　　　　 驻地工程师：            日期："]
[]
[]
[]
[]
[]
[{"$nulls":9}," "]

{"sheet":"610","index":9,"n_rows":18,"n_cols":13,"rows_kept":18,"merged":[[0,0,0,12],[1,0,1,12],[4,0,6,0],[4,2,6,2],[4,3,5,4],[4,5,5,6],[4,7,5,8],[4,9,5,10],[4,11,5,12],[17,0,24,5],[17,6,24,12]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表610                    标 线 喷 涂 检 验 表"]
["承包单位：",{"$nulls":10},"合同号："]
["监理单位：",{"$nulls":10},"编　号："]
["桩    号","左侧","损坏及脱落个数（%）","湿漆膜厚度（mm）",null,"标线宽度（mm）",null,"标线长度（mm）",null,"纵向间距（mm）",null,"横向偏位（mm）"]
[null,"或"]
[null,"右侧",null,"设 计","实 测","设 计","实 测","设 计","实  测","设 计","实  测","允许偏差","实  测"]
{"$rows_empty":10}
["自检结论： \n\n\n\n                                            \n\n                                               签字：                    日期：",{"$nulls":5},"监理评语：     \n\n\n\n                                                            \n\n                                                              签字：                    日期："]

{"sheet":"611","index":10,"n_rows":17,"n_cols":14,"rows_kept":17,"merged":[[0,0,0,13],[1,0,1,13],[2,11,2,12],[3,11,3,12],[4,0,6,0],[4,2,5,3],[4,4,5,5],[4,6,5,7],[4,8,5,9],[4,10,5,11],[4,12,5,13],[16,0,22,5],[16,6,22,13]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表611                    标 志 安 装 检 验 表"]
["承包单位：",{"$nulls":10},"合同号："]
["监理单位：",{"$nulls":10},"编　号："]
["位置（桩号）","左侧","立柱竖直度（mm/m）",null,"标志安装角度（°）",null,"标志下沿净空（mm）",null,"标志内侧距路肩边线距离（mm）",null,"立柱外边缘距路肩边线的距离（mm）",null,"立柱尺寸（mm）"]
[null,"或"]
[null,"右侧","允许偏差","实 测 值","允许偏差","实  测","设 计","实 测","设 计","实 测","设 计","实 测","设 计","实 测"]
{"$rows_empty":9}
["自检结论：    \n\n\n\n\n\n                                                      签字：                    日期：",{"$nulls":5},"监理评语：     \n\n\n\n\n\n                                                         签字：                    日期："]

{"sheet":"612","index":11,"n_rows":23,"n_cols":21,"rows_kept":23,"merged":[[0,0,0,18],[1,0,1,18],[2,0,2,5],[2,13,2,18],[3,0,3,5],[3,13,3,18],[4,1,4,4],[4,7,4,8],[4,9,4,11],[4,12,4,13],[4,14,4,18],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,13],[5,14,6,18],[7,0,8,0],[7,1,8,1],[7,14,8,18],[9,0,10,0],[9,1,10,1],[9,14,10,18],[11,0,12,0],[11,1,12,1],[11,14,12,18],[13,0,14,0],[13,1,14,1],[13,14,14,18],[15,0,16,0],[15,1,16,1],[15,14,16,18],[17,7,17,8],[22,9,22,10]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表612                                        护 栏 检 验 表",{"$nulls":18}," "," "]
["承包单位：",{"$nulls":12},"      合同号：",{"$nulls":6}," "]
["监理单位：",{"$nulls":12},"      编    号：",{"$nulls":6}," "]
["起 讫 桩 号"," ",{"$nulls":3},"部位",null,"代表路段",null," ",null,null,"检查时间",{"$nulls":6}," "," "]
["检 查 项 目","允许偏差","设 计 值","实    测    值",{"$nulls":10},"合 格 率",{"$nulls":4}," "," "]
[{"$nulls":19}," "," "]
["立 柱 竖 直 度（mm/m）",null," "," "," "," ",null,null," ",null," "," "," "," "," ",{"$nulls":4}," "," "]
[null,null," "," "," "," ",null,null," ",null," "," "," "," ",{"$nulls":5}," "," "]
["柱 顶 高 度（mm）",null," "," "," "," ",null,null," ",null," "," "," "," "," ",{"$nulls":4}," "," "]
[null,null," "," "," "," ",null,null," ",null," "," "," "," ",{"$nulls":5}," "," "]
["设计立柱中距（mm）",null," "," "," "," ",null,null," ",null," "," "," "," "," ",{"$nulls":4}," "," "]
[null,null," "," "," "," ",null,null," ",null," "," "," "," ",{"$nulls":5}," "," "]
["隔离栅顺直度（mm/m）",null," "," "," "," ",null,null," ",null," "," "," "," "," ",{"$nulls":4}," "," "]
[null,null," "," "," "," ",null,null," ",null," "," "," "," ",{"$nulls":5}," "," "]
["混 凝 土 强 度（MPa）",null," "," "," "," ",null,null," ",null," "," "," "," "," ",{"$nulls":4}," "," "]
[null,null," "," "," "," ",null,null," ",null," "," "," "," ",{"$nulls":5}," "," "]
["外观检查：",{"$nulls":6},"自检结论：",{"$nulls":12}," "]
[{"$nulls":20}," "]
[{"$nulls":20}," "]
[{"$nulls":20}," "]
[{"$nulls":20}," "]
[null,"签字：",null,null,"日期：",{"$nulls":4},"签字：",{"$nulls":3},"日期："]

{"sheet":"613","index":12,"n_rows":17,"n_cols":14,"rows_kept":17,"merged":[[0,0,0,13],[1,0,1,13],[2,10,2,12],[3,10,3,12],[4,0,6,0],[4,1,5,2],[4,3,5,8],[4,9,5,13],[6,1,7,1],[6,2,7,2],[6,3,6,4],[6,5,6,6],[6,7,6,8],[6,9,6,12],[6,13,8,13],[16,0,16,6],[16,7,16,13],[17,0,22,13]],"flags":["formulas_cached_only"]}
["山东省公路工程"]
["检表613                   通讯管道基坑基线检验表 "]
["承包单位：",{"$nulls":9},"                                合同号："]
["监理单位：",{"$nulls":9},"                                编　号："]
["桩     号","硅管（根）",null,"回填砂厚度（cm）",{"$nulls":5},"水泥砂浆（cm）"]
[]
[null,"下  层","上  层","下  层",null,"上  层",null,"侧  边",{"$nulls":5},"厚度（cm）"]
[{"$nulls":3},"设计","实测","设计","实测","设计","实测","a","b","c","d"]
{"$rows_empty":8}
["自检结论：    \n\n\n\n\n\n                                                       \n                                                          签字：                    日期：",{"$nulls":6},"监理评语：\n\n\n\n\n\n\n                                                  签字：                    日期："]